#
SHIFT CONTROL OPERATION [JA5AX-EL]

id051705106200

## Range Determination

• Each range is determined by operating the selector lever, and switching ON/OFF the switch in the TR switch internal circuit. The present range is detected according to the ON/OFF signal of the switch.
• The following switches are built into the TR switch, and determine each range when the switch is on.

  P position switch
  R position switch
  N position switch
  D range switch