#
PARAMETER IDENTIFICATION (PID) DATA MONITORING FUNCTION [FS5A-EL]

id050221100700
• The PID mode allows access to certain data values, analog and digital input and output, calculations and system state information.

## Monitor Item Table

Item | Definition | Unit/Condition | TCM terminal
--- | --- | --- | ---
DTCCNT | Number of DTC detected | - | N/A
DWN SW | Down switch | On/Off | 2F
ETC TCM | Engine coolant temperature | °C | °F | N/A
GEAR_SEL | Gear commanded by module | 1/2/3/4/5 | N/A
HTM_CNT | Indicates number of high oil temperature mode (ATF temperature at 130 °C {266 °F} or more) operations | - | N/A
HTM_DIS | Indicates travel distance after operation of high oil temperature mode (ATF temperature at 130 °C {266 °F} or more) | km | N/A
ISS | Intermediate shaft speed | RPM | 2L
LINEDES | Target line pressure | kPa | inHg | N/A
LPS | Pressure control solenoid control A signal in TCM | A | 1E 1G
LPS B | Pressure control solenoid control B signal in TCM | % | 1D
MNL SW | M range switch | On/Off | 2B
OP_SW_B | Oil pressure switch | On/Off | 2J
OSS | Output shaft speed | RPM | 2P
RPM TCM | Engine speed | RPM | N/A
SSA/SS1 | Shift solenoid A control signal in TCM | % | 1A
SSB/SS2 | Shift solenoid B control signal in TCM | % | 1B
SSC/SS3 | Shift solenoid C control signal in TCM | % | 1C
SSD/SS4 | Shift solenoid D control signal in TCM | On/Off | 1F
SSE_SS5 | Shift solenoid E control signal in TCM | On/Off | 1H
SSF_SS6 | Shift solenoid F control signal in TCM | On/Off | 1J
TFT | ATF temperature | °C | °F | 2M
TFTV | ATF temperature signal voltage | V | 2M
THOP | Throttle position signal in TCM | % | N/A
TR | Transaxle range | P/R/N/D | 2H
TR_SENS | TR switch signal voltage | V | 2H
TSS | Input/turbine speed | RPM | 2I 2K
UP SW | Up switch | On/Off | 2D
VPWR TCM | Battery voltage | V | 1K
VSS | Vehicle speed | KPH | 2P