#
PID/DATA MONITOR AND RECORD PROCEDURE

id092200800600

1. Connect SST (WDS or equivalent) to the vehicle DLC-2 16-pin connector.

2. Access and monitor PIDs using SST (WDS or equivalent).

## Monitor Item Table

• The PID/DATA monitoring items for the instrument cluster is as shown in the table below.
-: Not applicable

PID item | Definition | Unit/Condition | Terminal
--- | --- | --- | ---
CCNT_HE | Continuous codes | Number of continuous codes | -
ECT_GAUGE | Temperature gauge | °C | °F | 2W, 2X
ODO COUNT | Total distance | km | mile
SPDOMETER | Speedometer | km/h | mile/h
TACH | Tachometer | rpm