#
DTC C1414 [ABS (ABS/TCS)]

id040214805200

DTC | C1414 | ABS (ABS/TCS) unit mismatched installation
DETECTION CONDITION | • Detection of situation where vehicle-type or drive system input signal and ABS (ABS/TCS) HU/CM information remains incongruent through CAN information
POSSIBLE CAUSE | • Mismatched installation of ABS (ABS/TCS) HU/CM

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT ABS (ABS/TCS) HU/CM FOR MISMATCHED INSTALLATION • Verify ABS (ABS/TCS) HU/CM part number • Has a ABS (ABS/TCS) HU/CM with the correct part number been installed? | Yes | Go to the next step.
No | Replace with correct ABS (ABS/TCS) HU/CM part number, then go to Step 7.
2 | INSPECT RELATED WIRING HARNESS FOR MISMATCHED INSTALLATION • Verify wiring harness part number • Has a wiring harness with the correct part number been installed? | Yes | Go to the next step.
No | Replace with correct ABS (ABS/TCS) HU/CM part number, then go to next Step.
3 | Configulate ABS (ABS/TCS) HU/CM • Can ABS (ABS/TCS) HU/CM configulate properly? | Yes | Go to the next step.
No | Replace ABS (ABS/TCS) HU/CM
4 | VERIFY TROUBLESHOOTING COMPLETED • Make sure to reconnected all disconnect connectors. • Clear the DTC from the memory. See Clearing DTCs Procedures • Is same DTC present? | Yes | Replace ABS (ABS/TCS) HU/CM, then go to the next step.
No | Go to the next step.
5 | VERIFY AFTER REPAIR PROCEDURE • Is there any other DTC present? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | Troubleshooting completed.