#
DTC P0300 [L8, LF, L3]

id0102a1806500

DTC P0300 | Random misfire detected
--- | ---
DETECTION CONDITION | • The PCM monitors CKP sensor input signal interval time. The PCM calculates the change of interval time for each cylinder. If the change of interval time exceeds the preprogrammed criteria, the PCM detects a misfire in the corresponding cylinder. While the engine is running, the PCM counts the number of misfires that occurred at 200 crankshaft revolutions and 1,000 crankshaft revolutions and calculates the misfire ratio for each crankshaft revolution. If the ratio exceeds the preprogrammed criteria, the PCM determines that a misfire, which can damage the catalytic converter or affect emission performance, has occurred. Diagnostic support note • This is a continuous monitor (Misfire). • MIL illuminates if the PCM detects the misfire which affects emission performance in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM. • The MIL flashes if the PCM detects a misfire which can damage the catalytic converter during the first drive cycle. • PENDING CODE is available if the PCM detects the misfire which affects emission performance during first drive cycle. • FREEZE FRAME DATA is available. • DTC is stored in the PCM memory.
POSSIBLE CAUSE | • CKP sensor malfunction • CMP sensor malfunction • Ignition coil malfunction • Ignition system malfunction • MAF sensor contamination • Excess air suction in intake air system (between MAF sensor and intake manifold) • Fuel pump malfunction • Fuel pressure regulator (built-in fuel pump unit) malfunction • Fuel line clogged • Fuel filter clogged • Fuel leakage in fuel line • Fuel runout • Poor quality fuel • Purge control solenoid valve malfunction • PCV valve malfunction • EGR valve malfunction • Vacuum hoses damages or improper connection • Related connector and terminal malfunction • Related wiring harness malfunction • Insufficient compression • Variable valve timing control system improper (LF, L3)

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA AND DIAGNOSTIC MONITORING TEST RESULTS HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service information. If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY RELATED PENDING CODE OR STORED DTC • Turn the ignition switch off then to the ON position (Engine off). • Verify related pending code or stored DTCs. • Are other DTCs present? | Yes | Go to the appropriate DTC troubleshooting. (See DTC TABLE [L8, LF, L3].)
No | Go to the next step.
4 | VERIFY CURRENT INPUT SIGNAL STATUS (KEY TO ON/IDLE) • Access APP1, APP2, ECT, IAT, MAF, RPM, TP, and VSS PIDs using the WDS or equivalent. (See PCM INSPECTION [L8, LF, L3].) • Is there any signal that is far out of specification when the ignition switch is turned to the ON position and the engine idles? | Yes | Inspect suspected circuit and/or part according to inspection results. (See PCM INSPECTION [L8, LF, L3].) Then go to Step 20.
No | Go to the next step.
5 | VERIFY CURRENT INPUT SIGNAL STATUS UNDER TROUBLE CONDITION • Inspect the same PIDs as in Step 4 while simulating FREEZE FRAME DATA condition. • Is there any signal which causes drastic changes? | Yes | Inspect suspected circuit and/or part according to inspection results. (See PCM INSPECTION [L8, LF, L3].) Then go to Step 20.
No | Go to the next step.
6 | INSPECT CMP SENSOR • Inspect CMP sensor. (See CAMSHAFT POSITION (CMP) SENSOR INSPECTION [L8, LF, L3].) • Is CMP sensor normal? | Yes | Go to the next step.
No | Inspect installation condition and damage timing chain and gears for, repair the malfunctioning part. • If it is normal, replace the CMP sensor. Then go to Step 20.
7 | VERIFY CKP SENSOR INSTALLATION CONDITION • Inspect for CKP sensor looseness. • Is CKP sensor loosen? | Yes | Retighten the CKP sensor, then go to Step.
No | Go to the next step.
8 | INSPECT IGNITION COIL HARNESSES • Inspect the ignition coil related harness condition (intermittent open or short) for all cylinders. • Are harness conditions normal? | Yes | Go to the next step.
No | Repair suspected wiring harnesses, then go to Step 20.
9 | INSPECT IGNITION SYSTEM OPERATION • Carry out spark test. (See Spark Test) • Is strong blue spark visible at each cylinder? | Yes | Go to the next step.
No | Repair or replace malfunctioning part according to spark test result. Then go to Step 20.
10 | INSPECT MAF PID • Start the engine. • Access MAF PID using the WDS or equivalent. • Race the engine and verify that MAF PID changes quickly according to change in the engine speed. • Is MAF PID response normal? | Yes | Go to the next step.
No | Replace the MAF sensor, then go to Step 20.
11 | INSPECT EXCESSIVE AIR SUCTION IN INTAKE AIR SYSTEM • Inspect for air leakage at following: - Between the MAF sensor and throttle body - Between throttle body and intake manifold • Is there any malfunction? | Yes | Repair or replace suspected part, then go to Step 20.
No | Go to the next step.
12 | INSPECT FUEL LINE PRESSURE • Inspect fuel line pressure. (See FUEL LINE PRESSURE INSPECTION [L8, LF, L3].) • Is fuel line pressure normal? | Yes | Go to Step 14.
No | If the fuel line pressure is too low, go to the next step. If the fuel line pressure is excess high, replace the fuel pump unit, then go to Step 20.
13 | INSPECT FUEL LINE FROM FUEL PUMP TO FUEL DELIVERY PIPE • Visually inspect fuel line for fuel leakage. • Is there any fuel leakage? | Yes | Replace suspected fuel line, then go to Step 20.
No | Inspect fuel filters for following: • Foreign material or stain inside fuel filter (low-pressure side) Perform the following actions depend on the result above. • If foreign materials or stain is found inside fuel filter (low-pressure side), clean the fuel tank and filter (low-pressure side). • If normal, replace the fuel pump unit. Then, go to Step 20.
14 | INSPECT ENGINE COMPRESSION • Inspect engine compression. (See COMPRESSION INSPECTION [L8, LF, L3].) • Is it normal? | Yes | Go to the next step. (LF, L3) Go to Step 16. (L8)
No | Perform engine overhaul for repairs, then go to Step 20.
15 | INSPECT VARIABLE VALVE TIMING CONTROL SYSTEM OPERATION • Inspect variable valve timing control system operation. (See Variable Valve Timing Control System Operation Inspection [LF, L3]) • Does variable valve timing control system work properly? | Yes | Go to the next step.
No | Repair or replace malfunctioning part according to variable valve timing control system inspection results, then go to Step 20.
16 | INSPECT OPERATION OF PURGE CONTROL SOLENOID VALVE • Turn the ignition switch off. • Connect the vacuum pump to the purge control solenoid valve and apply vacuum to the solenoid. • Verify that the solenoid holds vacuum. • Turn the ignition switch to the ON position (Engine off). • Access the EVAPCP PID in SIMULATION TEST using the WDS or equivalent. • Set the duty value to 100 % for EVAPCP PID. • Apply vacuum while turning the solenoid from OFF to ON and simulating the EVAPCP PID with 100 % duty value. • Verify that the solenoid releases vacuum while the solenoid is turned ON. • Is the purge control solenoid valve operation normal? | Yes | Go to the next step.
No | Replace the purge control solenoid valve, then go to Step 20.
17 | INSPECT PCV VALVE OPERATION • Turn the ignition switch off. • Remove the PCV valve and inspect the valve operation. (See PCV VALVE INSPECTION [L8, LF, L3].) • Is the PCV valve operation normal? | Yes | Replace the PCV valve, then go to Step 20.
No | Go to the next step.
18 | INSPECT OPERATION OF EGR VALVE • Remove the EGR valve. • Visually inspect if the EGR valve is stuck open. • Is the EGR valve stuck open? | Yes | Repair or replace the EGR valve, then go to Step 20.
No | Go to the next step.
19 | INSPECT SEALING OF ENGINE COOLANT PASSAGE • Perform "ENGINE COOLANT LEAKAGE INSPECTION." (See ENGINE COOLANT LEAKAGE INSPECTION [L8, LF, L3, L3 Turbo].) • Is there any malfunction? | Yes | Repair or replace malfunctioning part according to inspection results. Then go to the next step.
No | Go to the next step.
20 | VERIFY TROUBLESHOOTING OF MISFIRE DTC COMPLETED • Make sure to reconnect all disconnected connectors. • Turn the ignition switch to the ON position (Engine off). • Clear the DTC from the memory using the WDS or equivalent. • Perform the KOER self-test. (See KOEO/KOER SELF TEST [L8, LF, L3].) • Is the misfire DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [L8, LF, L3].)
No | Go to the next step.
21 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [L8, LF, L3].) • Are any DTC present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [L8, LF, L3].)
No | Troubleshooting completed.