#
DTC TABLE [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)]

id0902e5837000

DTC | Description | Page
--- | --- | ---
Security light | Security light flashing pattern | WDS or equivalent
11 |  | B1681 | Coil antenna signal is not received. | (See SECURITY LIGHT: DTC 11 (WDS OR EQUIVALENT: DTC B1681))
12 |  | B2103 | Coil antenna failure. | (See SECURITY LIGHT: DTC 12 (WDS OR EQUIVALENT: DTC B2103))
13 |  | B1600 | ID number signal is not received. | (See SECURITY LIGHT: DTC 13 (WDS OR EQUIVALENT: DTC B1600))
B2431 | Transponder programming failure. | (See SECURITY LIGHT: DTC 13 (WDS OR EQUIVALENT: DTC B2431))
14 |  | B1602 | PCM received invalid format of ID number from transponder. | (See SECURITY LIGHT: DTC 14 (WDS OR EQUIVALENT: DTC B1602))
15 |  | B1601 | PCM received incorrect ID number from key (transponder). | (See SECURITY LIGHT: DTC 15 (WDS OR EQUIVALENT: DTC B1601))
21 |  | B1213 | Number of valid keys is below minimum. | (See SECURITY LIGHT: DTC 21 (WDS OR EQUIVALENT: DTC B1213))
- | - | B1342 | PCM is defective. | (See SECURITY LIGHT: DTC - (WDS OR EQUIVALENT: DTC B1342))

  Note

  • Perform the following if the security light stays on:

  - If engine stalls, go to symptom troubleshooting NO.11 "ENGINE STALLS/QUITS, ENGINE RUNS ROUGH, MISSES, BUCK/JERK, HESITATION/STUMBLE, SURGES" in. (See NO.11 ENGINE STALLS/QUITS, ENGINE RUNS ROUGH, MISSES, BUCK/JERK, HESITATION/STUMBLE, SURGES [L8, LF, L3].) (See NO.13 ENGINE STALLS/QUITS, ENGINE RUNS ROUGH, MISSES, BUCK/JERK, HESITATION/STUMBLE, SURGES [MZR-CD (RF Turbo)].)
  - If engine won't start, go to symptom troubleshooting NO.6 "CRANKS NORMALLY BUT WILL NOT START" in. (See NO.6 CRANKS NORMALLY BUT WILL NOT START [L8, LF, L3].)(See NO.8 CRANKS NORMALLY BUT WILL NOT START [MZR-CD (RF Turbo)].)
  - If engine condition is normal but light stays on, inspect for continuity between the following wiring harness and body ground: security light and PCM connector terminal 2W. Repair or replace the wiring harness.