#
STEERING LOCK UNIT INSPECTION

id092100800500

1. Measure the voltage or inspect for continuity according to the Terminal Voltage Table (Reference).

  • If the voltage is not as specified in the Terminal Voltage Table (Reference), inspect the parts under "Inspection item(s)" and related wiring harnesses.

2. If the system does not work properly even though the inspection items or related wiring harnesses do not have any malfunction, replace the steering look unit.

## Terminal Voltage Table (Reference)

Terminal | Signal name | Connected to | Measured condition | Voltage (V)/Continuity | Inspection item(s)
--- | --- | --- | --- | --- | ---
E | Push switch signal | Keyless control module | Start knob pressed | B+ | • Keyless control module • Related wiring harnesses
Start knob released | 1.0 or less
F | Power supply | Fuse | Under any condition | B+ | • Fuse • Related wiring harnesses
G | Key reminder switch signal | Keyless control module | Key inserted | B+ | • Keyless control module • Related wiring harnesses
Key removed | 1.0 or less
I | Power supply | Fuse | Under any condition | B+ | • Fuse • Related wiring harnesses
K | Serial communication | Keyless control module | Under any condition: Inspect for continuity to keyless control module. | Continuity detected | Related wiring harnesses
L | GND | Body ground | Under any condition: Inspect for continuity to GND. | Continuity detected | Related wiring harnesses