#
PID/DATA MONITOR TABLE

id080200800800

PID name (definition) | Unit/condition | Condition/specification | terminal
--- | --- | --- | ---
CONT_RCM (Number of continuous DTC) | - | • DTC is detected: 1-255 • DTC is not detected: 0 | -
CRSH_ST_D1 (Driver-side air bag sensor communication state) | OK/ FAULT | • Sensor normal: OK • Sensor communication error: FAULT | 2Z, 2AA
CRSH_ST_D2 (Driver-side air bag sensor circuit state) | OK/ FAULT | • Sensor normal: OK • Sensor internal circuit error: FAULT | 2Z, 2AA
CRSH_ST_P1 (Passenger-side air bag sensor communication state) | OK/ FAULT | • Sensor normal: OK • Sensor communication error: FAULT | 2B, 2C
CRSH_ST_P2 (Passenger-side air bag sensor circuit state) | OK/ FAULT | • Sensor normal: OK • Sensor internal circuit error: FAULT | 2B, 2C
D_PTENSFLT (Driver-side pre-tensioner seat belt circuit state) | SQ_LOWRES OPEN SHRT_B+ SHRT_GND Normal | • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness circuit open: OPEN • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness normal: Normal | 2P, 2S
DABAGR (Driver-side air bag module resistance) | ohm | Under any condition: 1.5-3.7 ohm | 1S, 1V
DR_CURTN (Driver-side curtain air bag module resistance) | ohm | Under any condition: 1.4-3.2 ohm | 2Y, 2V
DR_PTENS (Driver-side pre-tensioner seat belt resistance) | ohm | Under any condition: 1.5-3.1 ohm | 2P, 2S
DS_AB (Driver-side side air bag module resistance) | ohm | Under any condition: 1.4-3.2 ohm | 2M, 2O
DS_AB_ST (Driver-side side air bag module circuit state) | SHRT_B+ SHRT_GND OPEN SQ_LOWRES Normal | • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 2M, 2O
DS_CURT_ST (Driver-side curtain air bag module circuit state) | SHRT_B+ SHRT_GND OPEN SQ_LOWRES Normal | • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 2V, 2Y
DS1_STAT (Driver-side air bag module circuit state) | SHRT_GND SHRT_B+ OPEN SQ_LOWRES Normal | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 1S, 1V
DSB_P_ST (On demand driver-side pre-tensioner seat belt circuit state) | SQ_LOWRES OPEN SHRT_B+ SHRT_GND Normal | • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness circuit open: OPEN • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness normal: Normal | 2P, 2S
I_PAD_SW (PAD switch status) | On/ Off | • PAD switch is at PASS AIRBAG ON position: On • PAD switch is at PASS AIRBAG OFF position: Off | 1I
IG_V_2 (System IG1 voltage value) | V | • Ignition switch to ON position: B+ • Other: 0 V | 1W
OD_CRST_D1 (On demand driver-side side air bag sensor communication state) | OK/ FAULT | • Sensor normal: OK • Sensor communication error: FAULT | 2Z, 2AA
OD_CRST_D2 (On demand driver-side side air bag sensor circuit state) | OK/ FAULT | • Sensor normal: OK • Sensor internal circuit error: FAULT | 2Z, 2AA
OD_CRST_P1 (On demand passenger-side side air bag sensor communication state) | OK/ FAULT | • Sensor normal: OK • Sensor communication error: FAULT | 2B, 2C
OD_CRST_P2 (On demand passenger-side side air bag sensor circuit state) | OK/ FAULT | • Sensor normal: OK • Sensor internal circuit error: FAULT | 2B, 2C
OD_D_CURT (On demand driver-side curtain air bag module circuit state) | SHRT_B+ SHRT_GND OPEN SQ_LOWRES Normal | • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 2V, 2Y
OD_DAB1_ST (On demand driver-side air bag module circuit state) | SHRT_GND SHRT_B+ OPEN SQ_LOWRES Normal | • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 1S, 1V
OD_DSAB_ST (On demand driver-side side air bag circuit state) | SHRT_B+ SHRT_GND OPEN SQ_LOWRES Normal | • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 2M, 2O
OD_P_CURT (On demand passenger-side curtain air bag module circuit state) | SHRT_B+ SHRT_GND OPEN SQ_LOWRES Normal | • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 2A, 2D
OD_PAB1_ST (On demand passenger-side air bag module circuit state) | SHRT_GND SHRT_B+ OPEN SQ_LOWRES Normal | • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 1M, 1P
OD_PSAB_ST (On demand passenger-side side air bag sensor circuit state) | SHRT_B+ SHRT_GND OPEN SQ_LOWRES Normal | • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 2I, 2L
P_PTENSFLT (Passenger-side pre-tensioner seat belt circuit state) | SQ_LOWRES OPEN SHRT_B+ SHRT_GND Normal | • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness circuit open: OPEN • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness normal: Normal | 2G, 2J
PABAGR (Passenger-side air bag module resistance) | ohm | Under any condition: 1.4-2.9 ohm | 1M, 1P
PS_AB (Passenger-side side air bag module resistance) | ohm | Under any condition: 1.4-3.2 ohm | 2I, 2L
PS_AB_ST (Passenger-side side air bag sensor circuit state) | SHRT_B+ SHRT_GND OPEN SQ_LOWRES Normal | • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 2I, 2L
PS_CURTN (Passenger-side curtain air bag module resistance) | ohm | Under any condition: 1.4-3.2 ohm | 2A, 2D
PS_CURT_ST (Passenger-side curtain air bag module circuit state) | SHRT_B+ SHRT_GND OPEN SQ_LOWRES Normal | • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 2A, 2D
PS_PTENS (Passenger-side pre-tensioner seat belt resistance) | ohm | Under any condition: 1.5-3.1 ohm | 2G, 2J
PS1_STAT (Passenger-side air bag module circuit state) | SHRT_GND SHRT_B+ OPEN SQ_LOWRES Normal | • Related wiring harness short to ground: SHRT_GND • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness circuit open: OPEN • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness normal: Normal | 1M, 1P
PSB_P_ST (On demand passenger-side pre-tensioner seat belt circuit state) | SQ_LOWRES OPEN SHRT_B+ SHRT_GND Normal | • Air bag module circuit resistance low: SQ_LOWRES • Related wiring harness circuit open: OPEN • Related wiring harness short to power supply: SHRT_B+ • Related wiring harness short to ground: SHRT_GND • Related wiring harness normal: Normal | 2G, 2J