#
PID/DATA MONITOR INSPECTION [FS5A-EL]

id050221805600

1. Connect the WDS or equivalent to the DLC-2.

2. Measure the PID value.

  Note

  • Perform part inspection for the output device after TCM inspection.
  • The PID/DATA MONITOR function monitors the calculated value of the input/output signals in the TCM. Therefore, if a monitored value of an output device is out of specification, it is necessary to inspect the monitored value of the input device related to the output device control. Since an output device malfunction is not directly indicated as a malfunction of the monitored value for the output device, it is necessary to inspect the output device individually using methods such as the simulation function.

PID/DATA MONITOR AND RECORD function table

Monitor item (Definition) | Unit/Condition | Condition/Specification | Action | TCM terminal
--- | --- | --- | --- | ---
DTCCNT (Number of DTC detected) | - | • DTCs is detected: 1-255 • No DTCs are detected: 0 | Perform applicable DTC troubleshooting. (See DTC TABLE [FS5A-EL].) | N/A
DWN SW (Down switch) | On/Off | • M range, downshift: On • Other: Off | Inspect the selector lever component. (See SELECTOR LEVER COMPONENT INSPECTION.) | 2F
ECT TCM (ECT sensor) | °C | °F | Indicates engine coolant temperature | Inspect the ECT sensor. (See ENGINE COOLANT TEMPERATURE (ECT) SENSOR INSPECTION [L8, LF, L3].) Inspect the PCM (See PCM INSPECTION [L8, LF, L3].) | N/A
GEAR_SEL | 1/2/3/4/5 | 1GR: 1 2GR: 2 3GR: 3 4GR: 4 5GR: 5 | Inspect the following PIDs: SSA/SS1, SSB/SS2, SSC/SS3, SSD/SS4, SSD_SS5, SSF_SS6 | 1A, 1B, 1C, 1D, 1F, 1H, 1J
HTM_CNT | - | Indicates number of high oil temperature mode (ATF temperature at 130 °C {266 °F} or more) operations 0-255 | - | N/A
HTM_DIS | km | Indicates travel distance after operation of high oil temperature mode (ATF temperature at 130 °C {266 °F} or more) 0-2550 km | - | N/A
ISS (Intermediate shaft speed) | RPM | Indicates secondary gear revolution speed • Vehicle speed 0 km/h {0 mph}: 0 RPM • Vehicle speed 25 km/h {16 mph}: 200-230 RPM | Inspect the intermediate sensor. (See INTERMEDIATE SENSOR INSPECTION [FS5A-EL].) | 2L
LINEDES | kPa | inHg | Indicates target line pressure | Inspect the following PIDs: ISS, OSS, TFT, TFTV, THOP, TR, TSS | N/A
LPS (Pressure control solenoid A) | A | Change current value according to throttle opening angle | Inspect the pressure control solenoid A. (See SOLENOID VALVE INSPECTION (PRIMARY CONTROL VALVE BODY) [FS5A-EL].) | 1E, 1G
LPS B (Pressure control solenoid B) | % | 4GR→ 5GR: 99% • others: 0% | Inspect the pressure control solenoid B. (See SOLENOID VALVE INSPECTION (SECONDARY CONTROL VALVE BODY) [FS5A-EL].) | 1D
MNL SW (M range switch) | On/Off | • M range: On • Other: Off | Inspect the selector lever component. (See SELECTOR LEVER COMPONENT INSPECTION.) | 2B
OP_SW_B (Oil pressure switch) | On/Off | 1GR, 2GR or 3GR: On • Other: Off | Inspect the oil pressure switch. (See OIL PRESSURE SWITCH INSPECTION [FS5A-EL].) | 2J
OSS (Output shaft speed) | RPM | Indicates output shaft speed • Vehicle speed 0 km/h {0 mph}: 0 RPM • Vehicle speed 25 km/h {16 mph}: 200-230 RPM | Inspect the VSS. (See VEHICLE SPEED SENSOR (VSS) INSPECTION [FS5A-EL].) | 2P
RPM_TCM (Engine speed) | RPM | Ignition switch ON: 0 RPM Idle: 700-800 RPM | Inspect the TCM. (See TCM INSPECTION [FS5A-EL].) | N/A
SSA/SS1 (Shift solenoid A) | % | 4GR: 99% • others: 0% | Inspect the shift solenoid A. (See SOLENOID VALVE INSPECTION (PRIMARY CONTROL VALVE BODY) [FS5A-EL].) | 1A
SSB/SS2 (Shift solenoid B) | % | 1GR at D range: 99% • Others: 0% | Inspect the shift solenoid B. (See SOLENOID VALVE INSPECTION (PRIMARY CONTROL VALVE BODY) [FS5A-EL].) | 1B
SSC/SS3 (Shift solenoid C) | % | 1GR/2GR: 99% • Others: 0% | Inspect the shift solenoid C. (See SOLENOID VALVE INSPECTION (PRIMARY CONTROL VALVE BODY) [FS5A-EL].) | 1C
SSD/SS4 (Shift solenoid D) | On/Off | • P/N position, 4GR at D range, 1GR at M range: On • Others: Off | Inspect the shift solenoid D. (See SOLENOID VALVE INSPECTION (PRIMARY CONTROL VALVE BODY) [FS5A-EL].) | 1F
SSE_SS5 (Shift solenoid E) | On/Off | • TCC operating: On • TCC non operating: Off | Inspect the shift solenoid E. (See SOLENOID VALVE INSPECTION (PRIMARY CONTROL VALVE BODY) [FS5A-EL].) | 1H
SSF_SS6 (Shift solenoid F) | On/Off | 1GR/2GR/3GR/4GR: On 5GR: Off | Inspect the shift solenoid F. (See SOLENOID VALVE INSPECTION (SECONDARY CONTROL VALVE BODY) [FS5A-EL].) | 1J
TFT (Transaxle fluid temperature) | °C | °F | Indicates transaxle fluid temperature | Inspect the TFT sensor. (See TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR INSPECTION [FS5A-EL].) | 2M
TFTV (Transaxle fluid signal voltage) | V | • ATF 20 °C {68 °F}: Approx. 3.3 V • ATF 40 °C {104 °F}: Approx. 2.4 V • ATF 60 °C {140 °F}: Approx. 1.5 V | Inspect the TFT sensor. (See TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR INSPECTION [FS5A-EL].) | 2M
THOP (Throttle position sensor) | % | • CTP: 12% • WOT: 75% | Inspect the TP sensor. (See THROTTLE POSITION (TP) SENSOR INSPECTION [L8, LF, L3].) | N/A
TR (Transaxle range) | - | • P position: P • R position: R • N position: N • D range: D | Inspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [FS5A-EL].) | 2H
TR_SENS (TR switch) | V | • P position: 4.34-4.79 V • R position: 3.83-4.18 V • N position: 3.05-3.50 V • D range: 2.23-2.66 V | Inspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [FS5A-EL].) | 2H
TSS (Input/turbine speed) | RPM | Indicates Input/turbine speed • Ignition switch ON: 0 RPM • Idle: 700-800 RPM (P, N position) | Inspect the input/turbine speed sensor. (See INPUT/TURBINE SPEED SENSOR INSPECTION [FS5A-EL].) | 2I, 2K
UP SW (Up switch) | On/Off | • M range, upshift: On • Other: Off | Inspect the selector lever component. (See SELECTOR LEVER COMPONENT INSPECTION.) | 2D
VPWR_TCM (Battery voltage) | V | B+ | Inspect the main relay. (See RELAY INSPECTION.) | 1K
VSS (Vehicle speed) | KPH | • Vehicle speed 20 km/h {12.5 mph}: 20 KPH • Vehicle speed 40 km/h {25 mph}: 40 KPH | Inspect the VSS. (See VEHICLE SPEEDOMETER SENSOR (VSS) INSPECTION [JA5AX-EL].) | 2P