#
GLOW SYSTEM OPERATION [MZR-CD (RF Turbo)]

id0113f1103100
• When the PCM energizes the glow plug relay, the glow plug activates, the circuit from the battery to the glow plug is established, and power is supplied to the glow plug via the glow plug lead. Due to this, the glow plug is heated and the combustion chamber is warmed up.

.

1 | Battery
2 | Glow plug relay
3 | Glow plug lead
4 | Glow plug