#
DUAL-MASS FLYWHEEL FUNCTION [A26M-R, A26MX-R]

id0510001001b0
• The dual-mass flywheel has separated primary and secondary flywheel, and a torsional damper that is located inside the flywheel. Due to this structure, the transaxle primary shaft rotation can be stabilized, decreasing noise inside the transaxle (gear teeth rattling) created by engine speed fluctuation, and thereby greatly reducing vehicle booming noise also.

.

1 | Torsional damper
2 | Primary flywheel
3 | Secondary flywheel