#
REAR WIPER MOTOR REMOVAL/INSTALLATION [WGN]

id0919004755a4

1. Disconnect the negative battery cable.

2. Remove the rear wiper arm and blade. (See REAR WIPER ARM AND BLADE REMOVAL/INSTALLATION [WGN].)

3. Remove the liftgate lower trim. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION [WGN].)

4. Remove in the order indicated in the table.

1 | Connector
2 | Bolt
3 | Rear wiper motor
4 | Outer bushing

5. Install in the reverse order of removal.

6. Adjust the rear wiper arm and blade. (See REAR WIPER ARM AND BLADE ADJUSTMENT [WGN].)