#
SAS CONTROL MODULE FUNCTION

id081000101000

## Outline

• Based on the module configuration, operation (deployment) matching the actual type of air bag module or pretensioner seat belt setting variation can be controlled. If the module configuration is incomplete or incorrect, the on-board diagnosis function displays a DTC. (See ON-BOARD DIAGNOSTIC FUNCTION OUTLINE.) If the SAS control module is replaced, it is necessary to perform the module configuration to match the specifications of the vehicle in which it is being installed. Refer to the Workshop Manual for the procedure.