#
ELECTRICAL FAN CONTROL OPERATION [MZR-CD (RF Turbo)]

id0140f1104000
• The PCM operates cooling fan relay No.1 and No.2 as indicated in the table below.

Relay | Operation | Condition
--- | --- | ---
Cooling fan relay No.1 | ON | • Engine coolant temperature is above 100 °C {212 °F}. • Engine coolant temperature sensor is malfunctioning. • Accelerator pedal is depressed.
OFF | Except above
Cooling fan relay No.2 | ON | • Engine coolant temperature is above 105 °C {221 °F}. • A/C switch is on. • Engine coolant temperature sensor is malfunctioning. • Accelerator pedal is depressed.
OFF | Except above