#
MEASURES IN AUDIO SYSTEM

id0903a1887100

## [Separation control]

- Utilizing the characteristic of monaural reception that noise is relatively less striking than stereo reception, the audio system automatically changes the reception from stereo to monaural and lessens annoying noise when signals become weak or a multipass phenomenon occurs.

## [High tone control]

- When signals become weak or a multipath phenomenon occurs, the audio system restrains volume level in high frequency band and lessens annoying noise.