#
STARTING PROCEDURE FOR ON-BOARD DIAGNOSTIC TEST MODE

id0902f6358300

  Note

  • All DTCs displayed in the on-board diagnostic test mode should be entered in the Audio Repair Order Form.

1. Turn the ignition switch to the ACC or ON position.

2. Turn the POWER switch off.

3. While pressing the POWER button, simultaneously press the FM1/2 button and the MEDIA button for 2 s or more.

1 | FM1 button
2 | MEDIA button
3 | POWER button (with RDS)
4 | POWER button (without RDS)
5 | SEEK button (with RDS)
6 | SEEK button (without RDS)

  Note

  • If several DTCs are in the memory, they can be displayed using the SEEK button.

4. To stop the on-board diagnostic test mode, turn the ignition switch off.