#
AFTER SERVICE PRECAUTION [L3 Turbo]

id0114b4801900

  Warning

  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. When installing the fuel hose, perform "Fuel Leakage Inspection" described below.

## Fuel Leakage Inspection

  Warning

  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Always carry out the following procedure with the engine stopped.

  Caution

  • Connecting to the wrong check connector terminal may cause a malfunction. Carefully connect only to the specified terminal.

1. Short the check connector terminal F/P to body ground using a jumper wire.

2. Turn the ignition switch to the ON position to operate the fuel pump.

3. Pressurize the system in this manner for at least 5 min to be sure there is no leakage.

  • If there is fuel leakage, inspect the fuel hoses, hose clamps, and fuel pipe sealing surface, and replace if necessary.

4. After repair, assemble the system and repeat Steps 1 to 3.