#
CLUTCH SWITCH INSPECTION [MZR-CD (RF Turbo)]

id0140f1445400

  Note

  • Perform the following test only when directed.

## Continuity Inspection

1. Disconnect the negative battery cable.

2. Remove the clutch switch (See CLUTCH PEDAL REMOVAL/INSTALLATION)

3. Inspect continuity between the clutch switch terminals using an ohmmeter.

  • If the clutch switch is okay, but the CPP PID is out of specification, perform the "Circuit Open/Short Inspection"
  • If not as specified, replace the clutch switch.

Specification

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)])

2. Inspect for open/short circuit in the following wiring harnesses.

  • If there is open/short circuit, repair or replace wiring harnesses.

### Open circuit

  • Clutch switch terminal A and PCM terminal 109
  • Clutch switch terminal B and body ground

### Short circuit

  • Clutch switch terminal A and power supply
  • Clutch switch terminal A and body ground
  • Clutch switch terminal B and power supply