#
FRONT DOOR SPEAKER REMOVAL/INSTALLATION

id092000802200

1. Disconnect the negative battery cable.

2. Remove the front door trim.

3. Remove in the order indicated in the table.

1 | Screw
2 | Connector
3 | Front door speaker (See Front Door Speaker Installation Note)

4. Install in the reverse order of removal.

## Front Door Speaker Installation Note

1. Attach the speaker with the wiring harness placed in the groove of the door unit panel.

  Caution

  • If the speaker is attached with the harness placed outside of the groove, the wiring harness might be broken.