#
WOOFER REMOVAL/INSTALLATION

id092000805200

## 4SD

1. Disconnect the negative battery cable.

2. Remove the rear package trim.

3. Remove in the order indicated in the table.

1 | Screw
2 | Connector
3 | Woofer

4. Install in the reverse order of removal.

## 5HB, WGN

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Temporary spare tire cover
2 | Wing bult
3 | Connector
4 | Woofer

3. Install in the reverse order of removal.