#
VEHICLE SPEEDOMETER SENSOR (VSS) INSPECTION [JA5AX-EL]

id051705265000

## On-Vehicle Inspection

1. Disconnect the terminal component No.2 connector.

2. Measure resistance between the terminals A and B.

  • If not as specified, inspect the VSS sensor. (See Inspection of Individual Part.)

Vehicle speedometer sensor (VSS)

  Resistance: 513-627 ohms (ATF temperature: 20 °C {68 °F})

3. Connect the terminal component No.2 connector.

## Inspection of Individual Part

1. Remove the VSS sensor. (See VEHICLE SPEEDOMETER SENSOR (VSS) REMOVAL/INSTALLATION [JA5AX-EL].)

2. Measure resistance between the terminals of the VSS speed sensor.

  • If not as specified, replace the VSS sensor.
  • If it is normal, replace the harness.

Vehicle speedometer sensor (VSS)

  Resistance: 513-627 ohms (ATF temperature: 20 °C {68 °F})

3. Install the VSS sensor. (See VEHICLE SPEEDOMETER SENSOR (VSS) REMOVAL/INSTALLATION [JA5AX-EL].)