#
NO.2 VEHICLE MOVES IN N POSITION [JA5AX-EL]

id050305800700

2 | Vehicle moves in N position
DESCRIPTION | • Vehicle creeps in N position. • Vehicle creeps if brake pedal not depressed in N position.
POSSIBLE CAUSE | • If vehicle moves in N position, basically, malfunction is in ATX. Since a malfunction in sensor circuit or output circuit is cause of malfunction in ATX, inspect sensors, output circuit, and related harnesses. - Clutch burned (Low clutch, Low one-way clutch, Low and reverse brake) • Line pressure low • Malfunction of control valve body - Selector lever position disparity (Although the selector indicator shows N position, hydraulic circuit shows D range or R position) Note • Before following troubleshooting steps, make sure that Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Does vehicle creep when selector lever moved slightly in N position? | Yes | • Overhaul control valve body and repair or replace any defective parts. (See ATX Workshop Manual.) - If problem remains, replace or overhaul transaxle and repair or replace any defective parts. (See AUTOMATIC TRANSAXLE AND TRANSFER REMOVAL/INSTALLATION [JA5AX-EL].) (See ATX Workshop Manual.)
No | Inspect and adjust selector lever. (See SELECTOR LEVER INSPECTION.) (See SELECTOR CABLE ADJUSTMENT.)
2 | • Verify test results. - If okay, return to diagnostic index to service any additional symptoms. - If malfunction remains, inspect related Service Informations and perform repair or diagnosis. • If vehicle repaired, troubleshooting completed. • If vehicle not repaired or additional diagnostic information not available, replace TCM.