#
DTC B2867

id080200803100

DTC B2867 | SAS control module connector poor connection
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection with only detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • There is no continuity between poor connection detector bar terminals of SAS control module.
POSSIBLE CAUSE | • Poor connection of any SAS control module connectors • Malfunction of any SAS control module connectors • SAS control module malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY THAT ALL SAS CONTROL MODULE CONNECTORS ARE CONNECTED WITH SAS CONTROL MODULE Warning • Handling the air bag system components improperly can accidentally deploy the air bag modules and pre-tensioner seat belts, which may seriously injure you. Read the service warnings and cautions before handling the air bag system components. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.) • Turn ignition switch to LOCK position. • Disconnect the negative battery cable and wait for 1 min or more. • Turn up floor covering. • Are all SAS control module connectors securely connected? | Yes | Go to the next step.
No | Reconnect connector properly.
2 | INSPECT ALL SAS CONTROL MODULE CONNECTORS • Remove the column cover. • Disconnect the clock spring connector. • Remove the glove compartment. • Disconnect the passenger-side air bag module connector. • Disconnect the driver and passenger-side side air bag module connectors. • Disconnect the driver and passenger-side curtain air bag module connectors. • Remove the B-pillar lower trims. • Disconnect the driver and passenger-side pre-tensioner seat belt connectors. • Disconnect the all SAS control module connectors. • Are poor connection detector bars of all SAS control module connectors normal? | Yes | Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.)
No | Replace wiring harnesses.