#
BRAKE PEDAL INSPECTION

id041100801100

## Brake Pedal Height Inspection

1. Verify that the distance from the carpet to the center of the upper surface of the pedal pad is as specified.

Brake pedal height (reference value)

  L.H.D.: 187 mm {7.36 in}
  R.H.D.: 172 mm {6.77 in}

## Brake Pedal Height Adjustment

1. Loosen locknut B and turn the bolt A until it does not contact the pedal.

2. Loosen locknut D and turn rod C to adjust the height.

3. Tighten the bolt with locknut B.

Tightening torque

  9.8-14.7 N·m {100-149 kgf·cm, 116-130 in·lbf}

4. After adjustment, inspect the pedal play and the brake light operation.

## Brake Pedal Play Inspection

1. Depress the pedal a few times to eliminate the vacuum in the system.

2. Remove the spring pin, verify that the holes in the fork and in the pedal are aligned, and reinstall the pin. (See BRAKE PEDAL REMOVAL/INSTALLATION.)

3. Gently depress the pedal by hand until resistance is felt, and check the pedal play.

Brake pedal play

  0-3 mm {0-0.1 in}

## Brake Pedal Play Adjustment

  Caution

  • The brake switch may not operate normally after adjusting the pedal height. Whenever adjusting the pedal height, replace the brake switch with a new one.

1. Remove the spring pin and clevis pin. (See BRAKE PEDAL REMOVAL/INSTALLATION.)

2. Loosen locknut D and turn rod C to align the holes in the fork and in the pedal.

3. Install the clevis pin and the spring pin.

4. Tighten locknut D.

Tightening torque

  15.7-21.6 N·m {1.61-2.20 kgf·m, 11.6-15.9 ft·lbf}

5. Check the pedal height and the brake light operation.

## Pedal-to-floor Clearance Inspection

1. Start the engine and depress the brake pedal with a force of 588 N {60 kgf, 132 lbf}

2. Verify that the distance from the floor panel to the pedal pad center is as specified when the pedal is depressed.

  • If the distance is less than specified, inspect for air in brake system.

Brake pedal-to-floor clearance (Brake pedal when depressed at 588 N {60 kgf, 132 lbf})

  68 mm {2.7 in} or more