#
FRONT DRAIN HOSE INSTALLATION

id091500801400

  Caution

  • If the front drain hose is pinched or bent anywhere, the water in the hose may not discharge and enter the inside of the vehicle. During and after installation of the trims and the headliner, always make sure there is no interference with the front drain hose. Fix any problem if found.

1. Apply soapy water to the front drain hose inserting area.

2. Insert one end (the wider end) of the front drain hose into the sunroof frame.

3. Install the front drain hose to the clips, parallel to the pillar and free of slack.

4. Insert the front drain hose joint into the hinge pillar inner hole.

5. Install the headliner.(See HEADLINER REMOVAL/INSTALLATION [4SD, 5HB].)(See HEADLINER REMOVAL/INSTALLATION [WGN].)

6. Install the net anchor (WGN).

7. Install the assist handle.(See ASSIST HANDLE REMOVAL/INSTALLATION.)

8. Install the sunvisors.(See (SUNVISOR REMOVAL/INSTALLATION.)

9. Install the cargo compartment light (WGN).(See CARGO COMPARTMENT LIGHT REMOVAL/INSTALLATION [WGN].)

10. Install the rear map light.(See REAR MAP LIGHT REMOVAL/INSTALLATION.)

11. Install the front map light.(See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

12. Install the D-pillar trims (WGN).(See D-PILLAR TRIM REMOVAL/INSTALLATION [WGN].)

13. Install the C-pillar trims.(See C-PILLAR TRIM REMOVAL/INSTALLATION [4SD, 5HB].)(See C-PILLAR TRIM REMOVAL/INSTALLATION [WGN].)

14. Install the B-pillar upper trims.(See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

15. Install the A-pillar trims.(See A-PILLAR TRIM INSTALLATION.)

16. Install the sunroof seaming welt.