#
REAR TILT MOTOR INSPECTION

id091300800800

1. Disconnect the rear tilt motor connector.

2. Inspect the rear tilt motor operation when B+ is applied to the terminals as shown.

  • If not as specified, replace rear tilt motor.

Motor operation | Connection
--- | ---
B+ | GND
Up | 1A (1C) | 1C (1A)
Down | 1C (1A) | 1A (1C)

  ( ) :
R.H.D.

3. Connect battery positive voltage to front tilt motor terminal 2A and connect terminal 2B to ground.

4. Operate the front tilt motor and measure the voltage at terminals 2A and 2B.

  • If there is any malfunction, replace the rear tilt motor.