DSC ON-BOARD DIAGNOSIS [DSC]

id040220807400

On-Board Diagnostic (OBD) Test Description

• The OBD test inspects the integrity and function of the DSC and outputs the results when requested by the specific tests.
• On-board diagnostic test also:

  ― Provides a quick inspection of the DSC usually performed at the start of each diagnostic procedure.
  ― Provides verification after repairs to ensure that no other faults occurred during service.

• The OBD test is divided into 3 tests:

  ― Read/clear diagnostic results, PID monitor and record and active command modes.

Read/clear diagnostic results

  • This function allows you to read or clear DTCs in the DSC HU/CM memory.

PID/data monitor and record

  • This function allows you to access certain data values, input signals, calculated values, and system status information.

Active command modes

  • This function allows you to control devices through the WDS or equivalent.

Reading DTCs Procedure

1. Connect WDS or equivalent to the vehicle DLC-2 connector.

am6zzw00007604

2. Retrieve DTC by WDS or equivalent.

Clearing DTCs Procedures

1. After repairs have been made, perform the DTCs reading procedure.

2. Erase DTC by WDS or equivalent.

3. Ensure that the customer’s concern has been resolved.

PID/Data Monitor and Record Procedure

1. Connect WDS or equivalent to the vehicle DLC-2 connector.

am6zzw00007604

2. Access and monitor PIDs by WDS or equivalent.

Active Command Modes Procedure

  Note
  • When driving, the ABS motor and each valve automatically turn ABS_POWER on, and then each command on. ABS_POWER regulates the power supply for the ABS motor and 8 valves.

1. Connect WDS or equivalent to the vehicle DLC-2 16-pin connector.

am6zzw00007604

2. Turn the ignition switch to ON (Engine OFF) or start engine.

3. Activate active command modes using WDS or equivalent.

DTC Table

DTC | Diagnosis system component | Page
--- | --- | ---
WDS or equivalent
B1318 | DSC power supply | (See DTC B1318 [DSC].)
B1342 | DSC HU/CM | (See DTC B1342 [DSC].)
B1483 | Brake switch signal | (See DTC B1483, B1484, B1486 [DSC].)
B1484 | Brake switch signal | (See DTC B1483, B1484, B1486 [DSC].)
B1486 | Brake switch signal | (See DTC B1483, B1484, B1486 [DSC].)
B1627 | Reverse signal | (See DTC B1627 [DSC].)
B2477 | Module configuration | (See DTC B2477 [DSC].)
C1095 | Motor relay, pump motor | (See DTC C1095, C1096 [DSC].)
C1096 | Motor relay, pump motor | (See DTC C1095, C1096 [DSC].)
C1119 | Engine control system | (See DTC C1119 [DSC].)
C1125 | Brake fluid level sensor | (See DTC C1125 [DSC].)
C1140 | DSC HU/CM (pump) | (See DTC C1140 [DSC].)
C1145 | Right front ABS wheel-speed sensor | (See DTC C1145, C1155, C1165, C1175 [DSC].)
C1148 | Right front ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1155 | Left front ABS wheel-speed sensor | (See DTC C1145, C1155, C1165, C1175 [DSC].)
C1158 | Left front ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1165 | Right rear ABS wheel-speed sensor | (See DTC C1145, C1155, C1165, C1175 [DSC].)
C1168 | Right rear ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1175 | Left rear ABS wheel-speed sensor | (See DTC C1145, C1155, C1165, C1175 [DSC].)
C1178 | Left rear ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1186 | Fail-safe relay | (See DTC C1186, C1266 [DSC].)
C1194 | Left front pressure reduction solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1198 | Left front pressure retention solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1210 | Right front pressure reduction solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1214 | Right front pressure retention solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1233 | Left front ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1234 | Right front ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1235 | Right rear ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1236 | Left rear ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1242 | Left rear pressure reduction solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1246 | Right rear pressure reduction solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1250 | Left rear pressure retention solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1254 | Right rear ABS pressure retention solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1266 | Fail-safe relay | (See DTC C1186, C1266 [DSC].)
C1280 | Combined sensor | (See DTC C1280, C1730, C1951, C1952, C1959 [DSC].)
C1400 | Right front traction switch solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1410 | Left front traction switch solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1414 | DSC HU/CM | (See DTC C1414 [DSC].)
C1507 | DSC control | (See DTC C1507, C1508 [DSC].)
C1508*1 | DSC control | (See DTC C1507, C1508 [DSC].)
C1510 | Right front solenoid valve, motor or ABS wheel-speed sensor/sensor rotor | (See DTC C1510, C1511, C1512, C1513 [DSC].)
C1511 | Left front solenoid valve, motor or ABS wheel-speed sensor/sensor rotor | (See DTC C1510, C1511, C1512, C1513 [DSC].)
C1512 | Right rear solenoid valve, motor or ABS wheel-speed sensor/sensor rotor | (See DTC C1510, C1511, C1512, C1513 [DSC].)
C1513 | Left rear solenoid valve, motor or ABS wheel-speed sensor/sensor rotor | (See DTC C1510, C1511, C1512, C1513 [DSC].)
C1730 | Combined sensor | (See DTC C1280, C1730, C1951, C1952, C1959 [DSC].)
C1949*2 | Combined sensor | (See DTC C1949, C1950 [DSC].)
C1950*2 | Combined sensor | (See DTC C1949, C1950 [DSC].)
C1951 | Combined sensor | (See DTC C1280, C1730, C1951, C1952, C1959 [DSC].)
C1952 | Combined sensor | (See DTC C1280, C1730, C1951, C1952, C1959 [DSC].)
C1953 | Brake fluid pressure sensor | (See DTC C1953, C1954 [DSC].)
C1954 | Brake fluid pressure sensor | (See DTC C1953, C1954 [DSC].)
C1955 | Steering angle sensor | (See DTC C1955, C1956 [DSC].)
C1956 | Steering angle sensor | (See DTC C1955, C1956 [DSC].)
C1957 | Right front stability control solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1958 | Left front stability control solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1959 | Combined sensor | (See DTC C1280, C1730, C1951, C1952, C1959 [DSC].)
U0073 | CAN system communication error | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0100 | Communication error to PCM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0101*3 | Communication error to TCM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0114*2 | Communication error to 4WD control module | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0155 | Communication error to instrument cluster | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U2511*2 | Abnormal message from 4WD control module | (See DTC U2511 [DSC].)

*1 :Only vehicles with 2WD
*2 :Only vehicles with 4WD
*3 :Only vehicles with ATX

PID/DATA Monitor Table

PID Name (Definition) | Unit/Condition | Condition/Specification | Action | DSC HU/CM terminal
--- | --- | --- | --- | ---
ABS_LAMP (ABS warning light driver output state) | On/Off | • ABS warning light is illuminated: ON • ABS warning light is not illuminated: Off | Inspect ABS warning light. | —
ABSLF_I (Left front ABS pressure retention solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
ABSLF_O (Left front ABS pressure reduction solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
ABSLR_I (Left rear ABS pressure retention solenoid valve output state) | On/Off | • During ABS or EBD control: On/Off (solenoid valve is activated/deactivated) • Not ABS and EBD control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
ABSLR_O (Left rear ABS pressure reduction solenoid valve output state) | On/Off | • During ABS or EBD control: On/Off (solenoid valve is activated/deactivated) • Not ABS and EBD control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
ABSRF_I (Right front ABS pressure retention solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
ABSRF_O (Right front ABS pressure reduction solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
ABSRR_I (Right rear ABS pressure reduction solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
ABSRR_O (Right rear ABS pressure reduction solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
ABSPMPRLY (Motor relay output state) | On/Off | • Motor relay is activated: On • Motor relay is deactivated: Off | Inspect DSC HU/CM. (See DSC HU/CM INSPECTION.) | —
ABSVLVRLY (Fail-safe relay output state) | On/Off | • Fail-safe relay is activated: On • Fail-safe relay is deactivated: Off | Inspect DSC HU/CM. (See DSC HU/CM INSPECTION.) | —
ABS_VOLT (System battery voltage value) | V | • Ignition key at ON: B+ • Idle: Approx. 14—16 V | Inspect power supply circuit. (See DSC HU/CM INSPECTION.) | G
ACCLMTR*1 (Forward-G sensor input) | G | • Vehicle is stopped or driving at a constant speed: 0 G • Cornering to left: Changes between 0 G and 1.5 G • Cornering to right: Changes between 0 G and -1.5 G | Inspect combined sensor. (See COMBINED SENSOR INSPECTION.) | V
AWD_MSG*1 (Missing message from the 4WD control module) | Present/ Not Present | • Present: Circuit in the 4WD control module is normal. • Not Present: Circuit in the 4WD control module is abnormal. | Inspect 4WD control module. (See 4WD CONTROL MODULE INSPECTION [L3 Turbo]) Inspect DSC HU/CM. (See DSC HU/CM INSPECTION) | —
BOO_ABS (Brake pedal switch input) | On/Off | • Brake pedal is depressed: On • Brake pedal is released: Off | Inspect brake switch. (See BRAKE SWITCH INSPECTION.) | —
BRK_FLUID (Brake fluid level sensor input) | OK/Low | • Brake fluid is above LOW: OK • Brake fluid is below LOW: Low | Inspect brake fluid level. Inspect brake fluid level sensor. (See BRAKE FLUID LEVEL SENSOR INSPECTION.) | —
BRAKE_LMP (BRAKE system warning light output state) | On/Off | • BRAKE system warning light is illuminated: On • BRAKE system warning light is not illuminated: Off | Inspect BRAKE system warning light. | —
CCNTABS (Number of continuous codes) | — | DTC is detected: 1—255 DTC is not detected: 0 | Perform inspection using appropriate DTC. | —
IC_MSG (Missing message from the instrument cluster) | Present/ Not Present | • Present: Circuit in the instrument cluster is normal. • Not Present: Circuit in the instrument cluster is abnormal. | Inspect instrument cluster. (See INSTRUMENT CLUSTER INSPECTION) Inspect DSC HU/CM. (See DSC HU/CM INSPECTION) | —
LAT_ACCL (Lateral-G sensor input) | G | • Vehicle is stopped or driving straight: 0 G • Cornering to left: Changes between 0 G and 1.5 G • Cornering to right: Changes between 0 G and -1.5 G | Inspect combined sensor. (See COMBINED SENSOR INSPECTION.) | O
L_DSC_O (Stability control solenoid valve (LF-RR)) | On/Off | • Solenoid valve is activated: On • Solenoid valve is deactivated: Off | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
LF_WSPD (Left front ABS wheel-speed sensor input) | KPH, MPH | • Vehicle is stopped: 0 KPH {0 MPH} • Vehicle is driving: Indicates vehicle speed | Inspect ABS wheel-speed sensor/sensor rotor. (See FRONT/REAR ABS WHEEL-SPEED SENSOR INSPECTION.) | F, J
LR_WSPD (Left rear ABS wheel-speed sensor input) | KPH, MPH | • Vehicle is stopped: 0 KPH {0 MPH} • Vehicle is driving: Indicates vehicle speed | Inspect ABS wheel-speed sensor/sensor rotor. (See FRONT/REAR ABS WHEEL-SPEED SENSOR INSPECTION.) | N, Q
MCYLI P (Brake fluid pressure sensor input) | Pa | • Brake pedal is depressed: Changes between 0 Pa and 25.5 MPa | Inspect DSC HU/CM. (See DSC HU/CM INSPECTION.) | —
PCM_MSG (Missing message from the PCM) | Present/ Not Present | • Present: Circuit in the PCM is normal. • Not Present: Circuit in the PCM is abnormal. | Inspect PCM. (See PCM INSPECTION [L8, LF, L3].) (See PCM INSPECTION [L3 Turbo].) (See PCM INSPECTION [MZR-CD (RF Turbo)].) Inspect DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
PMPSTAT (Pump motor output state) | On/Off | • Pump motor activate: On • Pump motor not activate: Off | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
R_DSC_O (Stability control solenoid valve (RF-LR)) | On/Off | • Solenoid valve is activated: On • Solenoid valve is deactivated: Off | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
RF_WSPD (Right front ABS wheel-speed sensor input) | KPH, MPH | • Vehicle is stopped: 0 KPH {0 MPH} • Vehicle is driving: Indicates vehicle speed | Inspect ABS wheel-speed sensor/sensor rotor. (See FRONT/REAR ABS WHEEL-SPEED SENSOR INSPECTION.) | I, M
RPM (Engine speed signal input) | RPM | • Engine is stopped: 0 RPM • Engine is running: Indicates engine speed | Inspect PCM. (See PCM INSPECTION [L8, LF, L3].) (See PCM INSPECTION [L3 Turbo].) (See PCM INSPECTION [MZR-CD (RF Turbo)].) | —
RR_WSPD (Right rear ABS wheel-speed sensor input) | KPH, MPH | • Vehicle is stopped: 0 KPH {0 MPH} • Vehicle is driving: Indicates vehicle speed | Inspect ABS wheel-speed sensor/sensor rotor. (See FRONT/REAR ABS WHEEL-SPEED SENSOR INSPECTION.) | H, K
SWA_POS (Steering angle sensor input) | ° | • Steering wheel is in neutral position: 0 ° • Steering wheel is turned to left: Changes between 0 ° and -1,640 ° • Steering wheel is turned to right: Changes between 0 ° and 1,640 ° | Inspect steering angle sensor. (See STEERING ANGLE SENSOR INSPECTION.) | R, U, W, X
TC LVAL (Traction switch solenoid valve (LF-RR)) | On/Off | • Solenoid valve is activated: On • Solenoid valve is deactivated: Off | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
TCM_MSG*2 (Missing message from the TCM) | Present/ Not Present | • Present: Circuit in the TCM is normal. • Not Present: Circuit in the TCM is abnormal. | Inspect TCM. (See TCM INSPECTION [FS5A-EL].) (See TCM INSPECTION [JA5AX-EL].) Inspect DSC HU/CM. (See DSC HU/CM INSPECTION.) | —
TC RVAL (Traction switch solenoid valve (RF-LR)) | On/Off | • Solenoid valve is activated: On • Solenoid valve is deactivated: Off | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | —
TPI (Throttle position signal input) | % | • Closed throttle position: 0% • Wide open throttle: Changes between 0% and 100% | Inspect PCM and throttle position sensor. (See PCM INSPECTION [L8, LF, L3].) (See PCM INSPECTION [L3 Turbo].) (See THROTTLE POSITION (TP) SENSOR INSPECTION [L8, LF, L3].) (See THROTTLE POSITION (TP) SENSOR INSPECTION [L3 Turbo].) | —
TRAC_SW*3 (DSC OFF switch input) | On/Off | • DSC OFF switch is depressed: On • DSC OFF switch is released: Off | Inspect DSC OFF switch. (See DSC OFF SWITCH INSPECTION.) | AA
TRANSGR (Transaxle gear position input) | 1/2/3/4/5/6/R/N/Error | • Transaxle gear /selector lever position*4 1GR: 1 2GR: 2 3GR: 3 4GR: 4 5GR: 5 6GR: 6 Reverse: R Neutral: N When gear position estimation is disabled: Error | Inspect PCM. (See PCM INSPECTION [L8, LF, L3].) (See PCM INSPECTION [L3 Turbo].) (See PCM INSPECTION [MZR-CD (RF Turbo)].) Inspect TCM. (See TCM INSPECTION [FS5A-EL].) (See TCM INSPECTION [JA5AX-EL].) | —
YAW_RATE (Yaw rate sensor input) | °/s | • Vehicle is stopped or driving straight: 0 °/s • Cornering to left: Changes between 0 °/s and 150 °/s • Cornering to right: Changes between 0 °/s and -150 °/s | Inspect combined sensor. (See COMBINED SENSOR INSPECTION.) | T

*1 :Only vehicles with 4WD
*2 : Only vehicles with ATX
*3 : Only vehicles with L3 Turbo
*4 :The displayed gear position is an estimated value based on the vehicle wheel speed and engine speed (MTX)

Active Command Modes Table

Command Name | Definition | Operation | Note
--- | --- | --- | ---
ABS_POWER | Fail-safe relay | On/Off | Ignition key at ON (Engine OFF), and driving
LATACCEL | Lateral-G sensor initialization | TRUE/FALSE
LF_DSC_V | Stability control solenoid valve (LF-RR) | On/Off
LF_INLET | Left front ABS pressure retention solenoid valve | On/Off
LF_OUTLET | Left front ABS pressure reduction solenoid valve | On/Off
LF_TC_VLV | Traction switch solenoid valve (LF-RR) | On/Off
LR_INLET | Left rear ABS pressure retention solenoid valve | On/Off
LR_OUTLET | Left rear ABS pressure reduction solenoid valve | On/Off
PMP_MOTOR | ABS motor | On/Off
RF_DSC_V | Stability control solenoid valve (RF-LR) | On/Off
RF_INLET | Right front ABS pressure retention solenoid valve | On/Off
RF_OUTLET | Right front ABS pressure reduction solenoid valve | On/Off
RF_TC_VLV | Traction switch solenoid valve (RF-LR) | On/Off
RR_INLET | Right rear ABS pressure retention solenoid valve | On/Off
RR_OUTLET | Right rear ABS pressure reduction solenoid valve | On/Off
STAB_IND | DSC indicator light | On/Off
TRAC OFF | DSC OFF light | On/Off
YAWRATE | Yaw rate sensor initialization | On/Off