#
DIFFERENTIAL OIL REPLACEMENT [L3 Turbo]

id0314a4800200

1. Place the vehicle on level ground.

2. Remove the filler plug.

3. Remove the drain plug and drain the differential oil into a container.

4. Install a new washer and the drain plug, and tighten.

Tightening torque

  39.2-53.9 N·m {4.0-5.4 kgf·m, 29.0-39.7 ft·lbf}

5. Add the specified differential oil from the filler plug until the level reaches the brim of the plug hole.

Rear differential oil type

  Grade: API service GL-5
  Viscosity: SAE 80W-90

Rear differential oil capacity (approximate quantity)

  1.00 L {1.06 US qt, 0.88 Imp qt}

6. After filling with differential oil, perform oil level inspection.

7. Install a new washer and the drain plug, and tighten.

Tightening torque

  39.2-53.9 N·m {4.0-5.4 kgf·m, 29.0-39.7 ft·lbf}