#
FUEL PUMP RESISTOR INSPECTION [L3 Turbo]

id0114b4801300

## Resistance Inspection

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF, L3, L3 Turbo].)

2. Remove the fuel pump resister. (See FUEL PUMP RESISTOR REMOVAL/INSTALLATION [L3 Turbo].)

3. Verify that the continuity between the fuel pump resister terminal A and B is within the specification.

  • If not within the specification, replace the fuel resistor.

Fuel pump resistor continuity

  0.304-0.336 ohms (20 °C {68 °F})