#
IGNITION COIL REMOVAL/INSTALLATION [L8, LF, L3, L3 Turbo]

id0118008002a4

1. Disconnect the negative battery cable.

2. Remove the plug hole plate. (L8, LF, L3) (See PLUG HOLE PLATE REMOVAL/INSTALLATION [L8, LF, L3].)

3. Remove the charge air cooler. (L3 Turbo) (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

4. Remove in the order indicated in the table.

1 | Connector
2 | Ignition coil

5. Install in the reverse order of removal.