#
SAS CONTROL MODULE CONFIGURATION

id081000801500

1. Connect the SST (WDS or equivalent) to the DLC-2.

2. Input vehicle information following the directions on the screen.

3. Select "Module programming".

4. Select "Programmable Module Installation".

5. Select the following items and perform procedures according to directions on the screen.

Item

  "RCM"

6. Retrieve DTCs by the SST (WDS or equivalent), then verify that there is no DTC present.

  • If DTC is present, perform applicable DTC present.