#
DOOR SWITCH REMOVAL/INSTALLATION

id091800803400

## Front

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Screw
2 | Door switch
3 | Connector

3. Install in the reverse order of removal.

## Rear

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Screw
2 | Door switch
3 | Connector

3. Install in the reverse order of removal.