#
INTRUDER SENSOR OPERATION

id0914b5115400

1. When the theft-deterrent system is armed, the intruder sensor outputs a 2.45 GHz radio wave in the passenger compartment. The intruder sensor detects phase differences in radio waves (reflected waves) that are output and bounced off a target object.

2. When a phase difference in reflected waves occurs by movement in the vehicle (intruder), the CPU calculates the level of phase difference.

3. If the level of phase difference is higher than specified, the intruder sensor sends a detection signal to the theft-deterrent module.

.

1 | Target object
2 | Receiver
3 | Transmitter
4 | Phase detection area
5 | Oscillator
6 | CPU
7 | Detection signal output
8 | Theft-deterrent control module