#
CYLINDER HEAD (I) DISASSEMBLY [WITHOUT DIESEL PARTICULATE FILTER]

id0110f4500400

1. Disassemble in the order indicated in the table.

1 | No.3 engine mount bracket
2 | Water outlet
3 | Dipstick
4 | Bypass pipe
5 | Cylinder head cover
6 | Fuel injection pipe
7 | Fuel injection pipe
8 | Common rail
9 | EGR water cooler
10 | Injection pump
11 | Intake manifold
12 | Injection pump bracket
13 | Nozzle seal
14 | Side wall
15 | Injection nozzle bracket
16 | Injection nozzle
17 | Rocker arm and rocker arm shaft (SeeRocker Arm and Rocker Arm Shaft Disassembly Note)
18 | Rocker bridge
19 | Camshaft
20 | Breather pipe

## Rocker Arm and Rocker Arm Shaft Disassembly Note

1. Inspect the camshaft end play.

(See CAMSHAFT END PLAY INSPECTION [WITHOUT DIESEL PARTICULATE FILTER])

2. Inspect the camshaft oil clearance.

(See CAMSHAFT OIL CLEARANCE INSPECTION [WITHOUT DIESEL PARTICULATE FILTER])

3. Loosen the bolts in two or three steps in the order shown.