#
PROPELLER SHAFT INSPECTION ON VEHICLE [JA5AX-EL]

id0315a1800700

## Joint Play Inspection

1. Move the joint shaft by hand, and verify that there is no play.

If there is play, perform the following service operations.

  • Yoke: Universal joint replacement (See PROPELLER SHAFT DISASSEMBLY/ASSEMBLY [JA5AX-EL].)
  • Constant velocity joint: Propeller shaft replacement (See PROPELLER SHAFT DISASSEMBLY/ASSEMBLY [JA5AX-EL].)

## Propeller Shaft Runout Inspection

  Caution

  • Do not rotate the propeller shaft by starting the engine.

1. Shift the select lever to N position and release the parking brake.

2. Rotate the rear wheel by hand, and measure the propeller shaft runout at 9 points as shown in the figure.

  Limit
  0.4 mm {0.02 in}