#
STEERING SPECIFICATIONS

id060000100300

Item | Specification
--- | ---
Steering wheel | Outer diameter | (mm {in}) | 372 {14.6}
Lock-to-lock | (turns) | L8, LF, L3 (except 18inch wheel), MZR-CD (RF Turbo): 2.75 L3 (18 inch wheel), L3 Turbo: 2.65
Steering gear and linkage | Type | Rack-and-pinion
Rack stroke | (mm {in}) | L8, LF, L3 (except 18inch wheel), MZR-CD (RF Turbo): 146.8-148.8 {5.780-5.858} L3 (18 inch wheel), L3 Turbo: 141.6-143.6 {5.575-5.653}
Steering column and shaft | Shaft type | Collapsible
Joint type | 2-cross joint
Amount of tilt | (mm {in}) | 45 {1.8}
Amount of telescope | (mm {in}) | 50 {2.0}
Power steering system | Power assist type | Engine speed sensing
Power steering fluid | Type | M-III or equivalent (e.g. Dexron®II)
Fluid capacity* (approximate quantity) | 2WD MTX (L8, LF, L3 (except 18inch wheel)): 0.80 L {0.84 US qt, 0.70 Imp qt} 2WD MTX (L3 (18 inch wheel)): 0.82 L {0.87 US qt, 0.72 Imp qt} 2WD ATX (LF, L3 (except 18inch wheel)): 0.87 L {0.92 US qt, 0.77 Imp qt} 2WD ATX (L3 (18 inch wheel)): 0.89 L {0.94 US qt, 0.78 Imp qt} 4WD (L3, L3 Turbo): 0.89 L {0.94 US qt, 0.78 Imp qt} MZR-CD (RF Turbo): 0.86 L {0.91 US qt, 0.76 Imp qt}
(L {US qt, Imp qt})

  * :
When reservoir tank is at maximum volume