#
SELECTOR LEVER INSPECTION

id051800800500

1. Turn the ignition switch to the ON position (engine OFF).

2. With the brake pedal depressed, verify that there is a "click" at each range when shifted.

3. Verify that the selector lever can be shifted.

4. Verify that there is a "click" at each position when shifted from P position to M range.

5. Verify that the positions of the selector lever and the indicator are aligned.

  • If not as specified, adjust the TR switch.

6. Verify that the vehicle operates in each selected range.