#
PARAMETER IDENTIFICATION (PID) ACCESS [JA5AX-EL]

id050206250700

Monitor item table

Display on the tester | Definition | Unit/Condition | TCM terminal
--- | --- | --- | ---
24B_Duty | 2-4 brake solenoid valve control signal in TCM | % | 2V
BOO_TCM | Brake switch | On/Off | 1U
DTCCNT | Number of DTC detected | - | -
DWN_SW | Down switch | On/Off | 1S
ECT TCM | Engine coolant temperature | °C | -
FDPDTC | Pending code causing FFD storage | - | -
GEAR_SEL | Calculated gear range in TCM | 1st/2nd/3rd/4th/5th | -
HC_Duty | High clutch solenoid valve control signal in TCM | % | 2U
LPS | Pressure control solenoid control signal in TCM | % | 2Y
MNL_SW | M range switch | On/Off | 1AA
OSS | Intermediate sensor | RPM | 1K, 1X
RPM_TCM | Engine speed | RPM | -
SSA/SS1 | Shift solenoid A control signal in TCM | On/Off | 2W
SSB/SS2 | Shift solenoid B control signal in TCM | On/Off | 2T
SSC/SS3 | Shift solenoid C control signal in TCM | On/Off | 2X
TCCC | TCC solenoid valve control signal in TCM | % | 2S
TFT | ATF temperature | °C | 1B, 1F
THOP | Throttle position | % | -
TR | Transaxle range position | R/N/D | 1T, 1W, 1Z
TRD | Tr switch (D range switch) | On/Off | 1Z
TRR | TR switch (R position switch) | On/Off | 1W
TSS | Input/turbine speed sensor | RPM | 1N, 2F
UP_SW | Up switch | On/Off | 2C
VPWR_TCM | Battery voltage | V | 1P
VSS | Vehicle speed | KPH | 1V, 1M