#
REAR OIL SEAL REPLACEMENT [L8, LF, L3]

id0110a1800900

1. Remove the flywheel (MTX) or Remove the drive plate (ATX). (See CLUTCH UNIT REMOVAL/INSTALLATION [L8, LF, L3].) (See DRIVE PLATE REMOVAL/INSTALLATION [JA5AX-EL].)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Bolt
2 | Rear oil seal (See Rear Oil Seal Installation Note)

## Rear Oil Seal Installation Note

1. Apply silicone sealant to the mating faces as shown.

  Thickness:
  4.0-6.0 mm {0.16-0.23 in}

2. Apply clean engine oil to the new oil seal lip.

3. Install the SST to the non-woven fabric side of the rear oil seal.

4. From the back side of the rear oil seal, verify that there is no damage or separation in the lip area of the rear oil seal.

5. Install the rear oil seal to the engine as shown in the figure.

6. Tighten the rear oil seal bolts in the order as shown.

  Tightening torque:
  8.0-11.5 N·m {81.6-117.2 kgf·m, 70.9-101.7 in·lbf}