#
DRIVE BELT INSPECTION [MZR-CD (RF Turbo)]

id0110f1801500

  Note

  • Drive belt deflection/tension inspection is not necessary because of the use of the drive belt auto tensioner.

1. Verify that the drive belt auto tensioner indicator mark does not exceeds the limit.

  • If it exceeds the limit, replace the drive belt. (See DRIVE BELT REPLACEMENT [MZR-CD (RF Turbo)].)

2. Install the washer tank.