#
CLUTCH PEDAL ADJUSTMENT

id051000802600

## Clutch Pedal Height

1. Measure the distance from the upper surface of the pedal pad.

  • If not as specified, adjust the pedal height by turning adjustment bolt B and locknut A.

Clutch pedal height (with carpet)

  L.H.D. (L8, LF, L3, MZR-CD (RF-Turbo)): 216-222 mm {8.50-8.74 in} (Reference value)
  R.H.D. (L8, LF, L3, MZR-CD (RF-Turbo)): 229-235 mm {9.02-9.25 in} (Reference value)
  L3 Turbo: 210-216 mm {8.27-8.50 in} (Reference value)

## Clutch Pedal Free Play

1. Depress the clutch pedal by hand until clutch resistance is felt, and measure the pedal free play.

  • If not as specified, adjust the pedal free play
  by loosening locknut C and turning push rod D as necessary.

Clutch pedal free play

  1.0-3.0 mm {0.04-0.11 in}

Clutch pedal push rod free play

  0.1-0.5 mm {0.004-0.020 in} (Reference value)

## Clutch Pedal Disengagement Point

1. Apply the parking brake and fix the front and rear of the wheels with the wheel chocks.

2. Start the engine at idle.

3. Without depressing the clutch pedal, move the

shift lever slowly to the reverse position.

4. Hold the lever when the gear noise is heard.

5. Depress the clutch pedal slowly.

6. Hold the pedal when the gear noise stops (clutch pedal disengagement point).

7. Measure distance A (the distance from the clutch pedal disengagement point to the fully depressed position) and the pedal stroke.

8. Verify that they are within specification.

  • If distance A or the pedal stroke is out of specification, adjust the pedal height or the clutch pedal free play to specification.

Clutch pedal disengagement stroke

  Minimum: 20 mm {0.79 in} (Reference value)

Clutch pedal stroke

  140 mm {5.51 in} (Reference value)