#
WHEEL APRON PANEL COMPONENT INSTALLATION

D6E098053210B02

1. When installing new parts, position each part so that the section measurement aligns to the body dimension.

2. Drill holes for plug welds before installing new parts.

3. After temporarily installing new parts, make sure the related parts fit properly.

  Note

  • When replacing the wheel apron panel (front) and the suspension housing separately, weld 6 locations indicated by (A).