#
TRUNK END TRIM REMOVAL/INSTALLATION [4SD, 5HB]

id0917004624a1

## 4SD

1. Remove the fasteners.

2. Pull the trunk end trim upward, then disengage clips A, pins B, and hooks.

3. Remove the trunk end trim.

4. Install in the reverse order of removal.

## 5HB

1. Pull the trunk end trim upward, then disengage clips A, pins B, and hooks.

2. Remove the trunk end trim.

3. Install in the reverse order of removal.