#
NEUTRAL SWITCH INSPECTION [L3 Turbo]

id0140b6800800

  Note

  • Perform the following inspection only when directed.

## Continuity Inspection

1. Disconnect the negative battery cable.

2. Remove the neutral switch. (See MANUAL TRANSAXLE REMOVAL/INSTALLATION [G35M-R].)

3. Inspect for continuity between the neutral switch terminals using a tester.

  • If the neutral switch is normal, but PID value is out of specification, perform the "Circuit Open/Short Inspection".
  • If not as specified, replace the neutral switch.

Specification

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION [L3 Turbo].)

2. Inspect the following harnesses for an open or short circuit. (Continuity check)

### Open circuit

  • If there is no continuity, there is an open circuit. Repair or replace the wiring harness.
  - Neutral switch terminal B and PCM terminal 1W
  - Neutral switch terminal A and body ground

### Short circuit

  • If there is no continuity, there is a short circuit. Repair or replace the wiring harness.
  - Neutral switch terminal B and body ground