#
IGNITION KEY ILLUMINATION FUNCTION

id091800101300
• The illumination time of the ignition key illumination is controlled by the microcomputer in the BCM.
• When the ignition switch is in the LOCK position (or ACC) position and the driver's door is open, the ignition key illumination is illuminated.

1 | Key reminder switch
2 | Ignition key illumination bulb
3 | Microcomputer
4 | Front door switch (Driver's side)