#
COOLING FAN COMPONENT CONSTRUCTION [L3 Turbo]

id0112b21005b3
• The cooling fan component consists of the radiator cowling, cooling fans, cooling fan motors, and fan control module.
• Electric cooling fans No.1 and No.2, which operate according to the fan control signal sent from the PCM to the fan control module, have been adopted. Due to this, engine noise has been reduced and rapid engine warming-up is possible.
• Cooling fan motor No.1 and the fan control module cannot be separated because they are integrated.
• The radiator cowling and cooling fans are made of plastic for weight reduction.
• Coolant reserve tank can be removed from the radiator cowling.

.

1 | Cooling fan component
2 | Cooling fan No.1
3 | Cooling fan No.2
4 | Radiator cowling
5 | Coolant reserve tank
6 | Cooling fan motor No.1
7 | Cooling fan motor No.2
8 | Fan control module

Cooling fan, cooling fan motor specification

Item | Specification
--- | ---
No.1 | No.2
Cooling fan | Number of blades | 5 | 7
Outer diameter | (mm {in}) | 320 {12.6}
Cooling fan motor output | (W) | 160