#
STEERING COLUMN CONSTRUCTION

id061400100800
• A steering column equipped with a tilt / telescoping system has been adopted for all models for improved operability.
• The tilt system is adjustable by 45 mm {1.8 in} in the up / down direction, the telescoping system is adjustable by 50 mm {2.0 in} in the forward / backward direction.

1 | Tilt amount 45 mm {1.8 in}
2 | Telescope amount 50 mm {2.0 in}
3 | Tilt/telescope amount lever