#
DTC INSPECTION [ADVANCED KEYLESS SYSTEM]

id0902e2839400

1. Connect the SST (WDS or equivalent) to the vehicle DLC-2 16-pin connector.

2. Verify the DTC with the SST (WDS or equivalent).

3. If a DTC is indicated, perform on-board diagnostic referring to the DTC table.

## PID/Data Monitor and Record Procedure

1. Connect the SST (WDS or equivalent) to the vehicle DLC-2 16-pin connector.

2. Access and monitor PIDs using the SST (WDS or equivalent).