#
CLIMATE CONTROL UNIT REMOVAL

id074000801800

1. Disconnect the negative battery cable.

2. Disconnect the air mix and airflow mode wires from each wire clamp and link. (Manual air conditioner)

3. Remove the center panel. (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)

4. Remove the screws and climate control unit. (Full-auto air conditioner)

5. Release the hook and pull the climate control unit toward you. (Manual air conditioner)

6. Disconnect the climate control unit connectors and remove the climate control unit. (Manual air conditioner)