#
FUEL FILTER COMPONENT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

id0114f1777800

1. Disconnect the negative battery cable.

2. Complete the "BEFORE REPAIR PROCEDURE". (See BEFORE REPAIR PROCEDURE [MZR-CD (RF Turbo)].)

3. Remove in the order indicated in the table.

L.H.D.

R.H.D.

1 | Connector
2 | Fuel hose
3 | Installation nut
4 | Fuel filter body

4. Install in the reverse order of removal.

5. Complete the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].)

6. Start the engine and verify that fuel does not leak from the fuel system.

  • If fuel leaks, reinstall the fuel filter.